**Pricing Tables**

Table # **–** Irrigation Items

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Item Description | Unit of Measurement | Estimated Quantity | Unit Price | Total |
| IR101 | Construct Concrete Pad for Irrigation Servicing Components | each |  |  |  |
| IR102 | Supply and Install Backflow Prevention Assembly with Heat Trace Cable | each |  |  |  |
| IR103 | Supply and Install Backflow Prevention Assembly Enclosure | each |  |  |  |
| IR104 | Supply and Install 25 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation System Piping | metres |  |  |  |
| IR104 | Supply and Install 38 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation System Piping | metres |  |  |  |
| IR104 | Supply and Install 50 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation System Piping | metres |  |  |  |
| IR104 | Supply and Install 75 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation System Piping | metres |  |  |  |
| IR104 | Supply and Install 100 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation System Piping | metres |  |  |  |
| IR10# | Supply and Install ## mm Water Valve Chamber including Gate Valve as per [insert Local Municipality] for Region Irrigation | each |  |  |  |
| IR10# | Connection to Existing [or Proposed] Watermain for Region Irrigation | each |  |  |  |
| IR10# | [insert additional items for water source connections as needed] | xxx |  |  |  |
| IR201 | Supply and Install 25 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation Service | metres |  |  |  |
| IR201 | Supply and Install 38 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation Service | metres |  |  |  |
| IR201 | Supply and Install 50 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation Service | metres |  |  |  |
| IR201 | Supply and Install 75 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation Service | metres |  |  |  |
| IR201 | Supply and Install 100 mm Diameter Rigid PVC Conduit by Open Cut for Irrigation Service | metres |  |  |  |
| IR202 | Supply and Install 300 mm Diameter Concrete Handwell for Irrigation Service | each |  |  |  |
| IR203 | Construct 600 mm Diameter Concrete Pole Base with Anchorage Assembly for Irrigation Service | each |  |  |  |
| IR204 | Supply and Install 3.7 Metre Octagonal Steel Pole for Irrigation Service | each |  |  |  |
| IR205 | Supply and Install Ground Rod for Irrigation Service | each |  |  |  |
| IR206 | Supply and Install Equipment for Power Supply for Irrigation Service | each |  |  |  |
| IR207 | Supply and Install Buried Ground Wire for Irrigation Service | metres |  |  |  |
| IR208 | Supply and Install Wire and Receptacles for Power Supply to Irrigation Controller and Backflow Prevention Assembly Enclosure | each system |  |  |  |
| IR301 | Supply, Install and Configure Pedestal Mounted Controller with Cellular Cartridge and Rain/Freeze Sensor | each |  |  |  |
| IR302 | Supply and Install 25 mm Master Valve and Flow Sensor Assembly | each |  |  |  |
| IR302 | Supply and Install 38 mm Master Valve and Flow Sensor Assembly | each |  |  |  |
| IR302 | Supply and Install 50 mm Master Valve and Flow Sensor Assembly | each |  |  |  |
| IR303 | Supply and Install Mainline Piping and Control Wiring | metres |  |  |  |
| IR304 | Supply and Install Quick Coupling Valve with Swing Joint and Stabilizer | each |  |  |  |
| IR305 | Supply and Install 25 mm Drip Control Zone | each |  |  |  |
| IR305 | Supply and Install 38 mm Drip Control Zone | each |  |  |  |
| IR306 | Supply and Install Dripline Tubing | lump sum | 1 |  |  |
| IR30# | [insert additional items for irrigation system requirements as needed] | xxx |  |  |  |

Cash Allowances

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item #** | **Item Description** | **Estimated Quantity** | **Cash Allowance** | **Total Cash Allowance** |
| IR400 | Irrigation Service Connection to Power by Local Hydro Authority (Cash Allowance) | 1 | xxx |  |